Mark Jundy P. Juaton September 18, 2023

BSIT – IT3R8 Networking 2

**FEEDBACK FOR MODULE 1.1**

1. Which part of this module you found interesting? Why?

* Basic configuration on both Switch and Router. It was previously discussed in networking 1, therefore some parts of this module serve as a review.

1. Which part of this module you consider challenging? Why?

* Securing remote access to the switch SSH. It requires secured management connection a remote device to prevent threats.

**Reflection**

1. Why should you configure the vty password for the switch?

* To allow telnet access and secure the connection of the remote device and the switch.

1. Why change the default VLAN 1 to a different VLAN number?

* To shutdown unused ports as well as prevent unauthorized access.

1. How can you prevent passwords from being sent in plain text?

* Service password encryption.

1. Why configure a static MAC address on a port interface?

* To ensure

Mark Jundy P. Juaton September 18, 2023

BSIT – IT3R8 Networking 2

**FEEDBACK FOR MODULE 1.1**

1. Which part of this module you found interesting? Why?
2. Which part of this module you consider challenging? Why?

**Reflection**

1. In researching a network connectivity issue, a technician suspects that an interface was not enabled. What show command could the technician use to troubleshoot this issue?

* Show ip interface brief

1. In researching a network connectivity issue, a technician suspects that an interface was assigned an incorrect subnet mask. What show command could the technician use to troubleshoot this issue?